|  |  |
| --- | --- |
| **Draft Determination Publication** | |
| **Network Queries** | |
| **Network Reference number** | SGN\_DDQ\_Q09 (High Priority) |
| **Licence** | SGN |
| **Topic/Activity:** | Repex - Mains Decommissioning Workloads (Southern & Scotland) |
| **Question:** | Relating to draft\_determinations\_-\_sgn\_annex.pdf  The only details we have received within the draft determination documents on Repex mains decommissioning lengths for GD2 is related to the Tier 1 iron PCD (SGN Annex - tables 12 & 13 on pages 14 & 15).  Please can you provide further details on the GD2 allowed / disallowed mains decommissioning lengths for all Repex mains categories and the methodology used to adjust these lengths?  This information is essential for us to provide an effective assessment of the draft determination in a timely manner. Without this information we are unable to assess whether we agree with the assessment made or not. |
| **DDQ raised by** | Danny Symes |
| **Date query raised** | 23/07/2020 |
| **Expected response date** | 30/07/2020 |
| **Ofgem Response:**  For both SGN networks other than Tier 1, which has been partially disallowed, the other mains categories have been either fully disallowed or fully allowed as described in chapter 3 of the draft determinations SGN annex. For the fully allowed workloads of these remaining categories, the detailed breakdown is as per the SGN submissions. | |
| **Attachments:** | |