**Data**

**Issues of concern Re data submitted and used by CORA Platform**

1. How do the FRS and the GDN decide whether or not to test for CO?
2. When testing is undertaken exactly what steps are taken before, during and after testing by the FRS and GDN?
3. If testing is not undertaken, what steps are taken?
4. If testing is undertaken is there a test of the air first:-
5. As found?
6. With all carbon-based fuelled appliances off at the time?
7. Then possibly with one carbon based fuelled appliance on?
8. Then add another and test etc.?
9. Are the emissions from each appliance tested for CO?
10. If CO is found are the parts per million (PPM) of CO found given to those exposed or who might have been exposed in writing/digitally for their medics?
11. If CO found are those exposed or might have been exposed merely told to ‘seek medical advice’? In our experience most medics know little or nothing about CO.
12. Are those exposed even capable of taking in this advice?
13. Is there any follow up at all?
14. If low or no CO is found what happens next? Do the FRS and/or GDN just leave? We suggest that a CO alarm to EN 50291 is left at the premises and also a CO logger (such as the one by Lascar) and a further visit made.
15. What is low CO? What level is ignored?