|  |  |  |
| --- | --- | --- |
| **Cadent Draft Determination** | | |
| **DD Query** | | |
| **SQ Reference number** | CADENT\_DDQ\_13 | |
| **Document Name** | Technical Annex – RIIO-GD2 Engineering Justification Paper Reviews Annex (QEM) | |
| **Topic/Activity:** | EJP Annex – Page 20, 5.3 Capex paragraph 5. | |
| **Question:** | Please give additional detail behind the statement “Crossings volumes include pipe remediation in all cases”. Please define the meaning and scope of a “pipe remediation”.  Crossing interventions may be on the coating, the installation of an Access Deterrent Measure (ADM) or a combined intervention of coating and ADM. Are you using the term pipe remediation to cover all these scenarios? | |
| **DDQ raised by** | Simon Brown | |
| **Date Sent** |  | |
| **Response Due Date** | 20/07/20 | |
| **Response Received** |  | |
| Pipe remediation in the draft determination report should be interpreted as painting or coating of the over-crossing pipe section, and not the access deterrent measure (ADM). | | |
| Attachments: | | |